SPECIFICATION TEXT PROPOSAL 
Secumat® Green 60G5 
		
Pos.: ……. Quantity: …..…… Unit Price: ……………. Total Price: ………………… 
Geonatural erosion control mat, Secumat® Green 60G5 or equivalent, manufactured by Naue GmbH & Co. KG, to be used as a biodegradable erosion control system. The scope includes supply and installation in accordance with the project design, layout and the manufacturer’s installation guidelines.

Secumat® Green 60G5 is a temporary, three-dimensional erosion control mat designed to consistently reduce soil erosion caused by rainfall and surface runoff.
The product consists of a naturally UV-stabilised, extruded randomly oriented filament layer, providing soil and root zone stabilization. The filament thickness and the mass per unit area form an artificial root zone across the layer thickness. Soil particles become embedded within the structure while plant roots can grow through the mat.

Quantities are based on the area to be covered. Material for overlapping and cut-off must be included.

The following parameters must be considered for proof of equivalency:

Technical data:

Complete product:

Raw material:							Biobased raw material “G5”

Filament thickness:			approx. 1.1 mm

Thickness			
(according to DIN EN ISO 9863-1):				approx. 12.0 mm

Mass per unit area							
(according to DIN EN ISO 9864):					600 g/m2

Colour:								kaki

Roll dimensions:

Width x Length:							2.00 m x 40 m

Diameter:								80 cm

Weight:								48 kg

Required documentation to be submitted with the tender:

•	Factory production control certificate for the product according to DIN 18200
•	Certified quality management system according to DIN EN ISO 9001:2015
•	Certified environmental management system according to DIN EN ISO 14001:2015
•	Certified energy management system according to DIN EN ISO 50001:2011
•	Proof of enviornmental compatibility of the product
•	The product must be covered within two weeks after installation. However, immediate covering may be required depending on project specific conditions.

Optimal fixing:

The Secumat® Green 60G5 shall be fixed to the ground with sustainably sourced hardwood pins referred to as Secumat® Green PinW 30.

Proof of Delivery (POD)
Secumat® Green 60G5
Naue GmbH & Co. KG
Gewerbestraße 2
32339 Espelkamp
GERMANY
Tel.: +49 5743 / 41-0
E-Mail: info@naue.com
www.naue.com  							Status: 01.08.2025