Author: Besser, Jörn
Last saved by: Hoyme, Dr. Helge
Company: HP

SPECIFICATION TEXT 
Secutex^® Green 120G1 GRK 5

Pos.: ……. Quantity: …..…… Unit price: ……………. Total price: ………………… 

Innovative protection, separation and filter nonwoven Secutex® Green 120G1 GRK 5, made of uniform fibres from renewable raw materials, biodegradable, produced by Naue GmbH & Co. KG or equivalent and installed professionally. The protective nonwoven fabric fulfils the requirements regarding grammage and puncture force of German geotextile robustness class 5 according to the FGSV bulletin on the use of geosynthetics in earthworks for road construction.

Secutex® Green 120G1 GRK 5 is a biodegradable, single-layer, needle-punched staple fibre protection, separation and filter nonwoven.

The following parameters are to be observed for the proof of equivalence, considering the tolerance specifications:

Tecnical data:

Mass per unit area:	1,200 g/m² (≥1,080 g/m²)
(acc. to DIN EN ISO 9864)

Thickness: 	7.0 mm	 (≥6.3 mm)
(acc. to DIN EN ISO 9863-1)

German Geotextile Robustness Class 5 	fulfilled
(acc. to FGSV M Geok E:
puncture resistance ≥ :3.5kN; mass per unit area ) ≥ 300 g/m²)	

Puncture resistance:	≥ 5,000 N 
(acc. to DIN EN ISO 12236)

Characteristic opening size:	45 µm
(acc. to DIN EN ISO 12956)

Detector tested:	yes

Properties raw material:	renewable and biodegradable 

Certifications

The following certificates (or comparable) to prove complete biodegradability under the respective boundary conditions specified in the currently valid standards for obtaining the certificates must be submitted

OK compost INDUSTRIAL of TÜV Austria
OK compost HOME of TÜV Austria
OK biodegradable SOIL of TÜV Austria
OK biodegradable WATER of TÜV Austria
OK biodegradable MARINE of TÜV Austria

Seedling certificate following EN 13432

Proof of delivery
Secutex^® Green 120G1 GRK 5   
Naue GmbH & Co. KG
Gewerbestraße 2
32339 Espelkamp-Fiestel
Germany
Tel.: +49 57 43 41 - 0
Fax: +49 57 43 41 - 240
E-Mail: info@naue.com
www.naue.com

page  of 					Status: 2022-03-03